Decking Plan

Purpose:

To build a decking and the outline the seating area within the permitted boundaries, where the sitting area is up 6 m length, 1.5m width and the high is 20cm.

Loudoun Road the decking is built cover with industrial wasted bins and when the wind blows all the rubbish is accumulated outside, this commercial premises which is not attractive neither for the shoppers or the people seating outside nor in inhabitancy of the above furthermore the wind time to time even pushes the waste inside the premises affecting the business operation, the decking has provided a shield against this blown waist.

The decking not only this decking preventing the rubbish be accumulated at the outside premises it has also created aesthetically pleasing seating area, green and organic asthenosphere and look to the area.

Location:

Decking to be built outside of the shop on the license area allocated for tables and chairs. Please see floor plan.

Type:

Wooden decking

Temporary structure easy to remove

When: 01/08/2022

Duration: 1 day from 8am until 17:00

Preparation:

Designated area to be close to public.

All wooden decking pieces will arrive to the side pre-cut, with the correct dimensions, the team will need only to install.

Decking wood will arrive at 7am before the shop opens to public and it will be storage inside the shop.

The team to build the decking ill arrive at 8am

Dimension:

Length: 6m

Width: 1.5m

Depth: 20mm