|  |  |
| --- | --- |
| LOCATION / PROJECT | 61-65 Charlotte Street  |
| HAZARD / WORK ACTIVITY ASSESSED | Use of Dust Producing Tools/ Completion of Dust Producing Activities  |
| H = HIGH RISK, M = MEDIUM RISK, L = LOW RISK, I = INSIGNIFICANT |
| SIGNIFICANT RISKS | H | M | L | I | WHO MAY BE HARMED |
| 1: Respiratory Diseases | X  |  |  |  | EMPLOYEES | X  |
| 2: Escape of dust into the atmosphere  | X  |  |  |  | SUBCONTRACTORS | X  |
| 3: Nuisance dust affecting neighbours  |  | X  |  |  | OFFICIAL VISITORS | X  |
| 4: Emissions from plant |  | X  |  |  | GENERAL PUBLIC | X  |
| 5:  |  |  |  |  | NEIGHBOURS | X  |
| 6:  |  |  |  |  |  |  |
| 7:  |  |  |  |  |  |  |
| 8 |  |  |  |  |  |  |
| CONTROL MEASURES |
| Wet cutting shall be employed when cutting all masonry/ concrete.LGF slab to have water applied via hosepipe during “breaking out”.Direct extraction to be fitted to circular/ table saws.Damping down to be employed when sweeping dusty areas.Face fit masks to be worn when completing dusty work.Windows and doors to be kept closed during dust producing activities.Neighbours to be informed when dust producing activities are planned to allow them to close their windows.Regular cleaning of neighbouring doors and windows to be introduced.Bunded boxes or skips will be provided for washing out of concrete.Scaffold will be enclosed with “Monarflex” sheeting to help contain any residual dust. |
| RESIDUAL RISK | LOW |
| INFORMATION, INSTRUCTION AND TRAINING |
| Only trained Operatives will change/mount abrasive wheels and discs. |
| PERSONAL PROTECTIVE EQUIPMENT |
| SAFETY HELMET | X  | EAR DEFENDERS | X  |
| SAFETY BOOTS | X  | RESPIRATORY PROTECTION | X  |
| GOGGLES / VISOR | X  | GLOVES  | X  |
| OVERALLS |  | EAR PLUGS |  |
| HI-VIZ | X  |  |  |
| AUTHORISATION |
| COMPLETED BY | SIGNATURE | DATE |
| South Downs Safety | scan0002 | 04.08.16 |