**21 Jeffrey’s Street NW1 9PS**

There are 3 double glazed windows that you have asked to be reinstated as single pane

Sitting room 94cms x 179cms

Basement 186cms x 117cms

Top bathroom 61cms x 117cms

Photographs attached

The attached adobe drawing demonstrates the existing double glazed units being replaced with single pane

Description of works,

Carefully remove double glazed units,

supply and fit a timber packer to each aperture,

then re glaze aperture with a single pane of 4mm float glass,

putty fronted.

Replace weights with correct weights, where applicable.

