**Specification of Aluminium Products:**

* **Profile:**✓Aluminium Cortizo System (Sliding Doors,)
* **All Gaskets -** Black
* **Powder Coated:** RAL 7016 (Anthracite Grey)
* **Type of profile:** Direct Fix(doors& windowfit directly into the brick)
* **Thermally broken profile:** Thermal barrier resist the transfer of cold from outside to the inside of the frame
* **Multipoint Locking System:** Fully comply with insurance requirements
* **Trickle Ventilators:** tested in accordance witch BS EN 13141:2004 (Ventilation for building)
* **Handle Cortizo:** Lever Lock & Barrel inside only
* **Hardware (Hinges & Handle):** Black or Satin (Satin Silver – Smart)**– TO BE CONFIRMED**
* **Glass:**4mm Soft Coat – Inner Pane/20mm Black Warm Edge Spacer, ARGON Filled/4mm Clear Glass – Outer Pane – Highest performing Insulated Glass Units (IGU)
* **Glass (Cortizo System):TO BE CONFIRMED**

o IGU to comply with document L (conservation of fuel and power)

o Safety Glass (Toughened) wherever required to comply with BS 6206 (Safety Glazing in Critical Location)

o Units are certified to the highest industry standards including BS EN 1279 parts 2, 3 and 6

2no of Aluminium Sliding Doors, Powder Coated: RAL 7016 (Anthracite Grey) – **Cortizo System (20mm Slim Interlock) Please Note:**

**Doors & Windows profiles differ from one another. Every door/ window system has different handles.**