**Installation & Maintenance for Biodiverse Roof**

**Installation**

1. Apply Waterproof membrane to roof
2. Apply protective root barrier
3. Fit perma-seal 20p to roof
4. Fit growing substrate
5. Plant & seed roof
6. Fit guttering & rainwater collection system

**Maintenance**

Twice a year cut and remove the seasons growth to encourage the spread of seed for the next season and remove any dead unsightly flower heads. Drainage channel and gutter clearance to remove any unwanted debris or leaf litter will also be carried out regularly.