NAGANJOHNSON ARCHITECTS  
2 Pontypool Place   
London SE1 8QF

020 7633 0200

[www.naganjohnson.co.uk](http://www.naganjohnson.co.uk/)

Application ref: 2020/3405/P

In response to conditions 4 and 5 b) for the above application please see below information and the following enclosed drawings and documents:

**Drawings**

PROV\_PP\_180\_2021 07 21 – 1:10 plan of extension

PROV\_PP\_181\_2021 07 21 – 1:10 Roof plan of extension

PROV\_PP\_185\_2021 07 21 – 1:10 (long) detailed section of extension

PROV\_PP\_186\_2021 07 21 – 1:10 (short) detailed section of extension

PROV\_PP\_186\_2021 07 21 – 1:10 (short) detailed section of extension

**Literature**

Bauder Single Ply System Technical Guide

Bauder Extensive Green Roof System Maintenance Procedure

Bauder Flora Seed Mix Range

VM Zinc Standing Seam

The key Materials are:

**Living Roof / Extensive green roof system**

The green roof is to be a Bauder system. Using a Bauder single ply membrane. Please refer to the attached literature.

The living roof with be planted with using Bauder Flora 5 Seed Mix GB ‘Urban’. The seeds will be saw by hand.

Table

Description automatically generated

Graphical user interface, application

Description automatically generated

Text

Description automatically generated

The Living roof will be maintained in accordance with Bauder ‘General maintenance, Green Roof Extensive System’, which is attached for reference.

**Stone**

The stone is to be Valanges limestone. Fabricated and installed by the Stonemasonry Company.

[The Stonemasonry Company Ltd](https://www.thestonemasonrycompany.co.uk/)

**Zinc**

The zinc is to be standing seam **VM Zinc Pigmento in Storm Grey**. Installed in accordance with the attached literature.

Graphical user interface, website

Description automatically generated