**External Wooden Door Specification**

**Standards**

* All materials and workmanship shall comply with the relevant British Standard or Code of Practice unless amended herein.
* BS 459, Parts 3 and 4 Wooden doors
* BS EN 942 Timber in joinery - General classification of timber quality
* BS 1186 : Part 2 Specification for workmanship
* BS 4787 : Part 1 Internal and external wooden door sets, door leaves and frames

**Materials & Workmanship**

* A standard softwood such as pine or redwood will be used for both the frame and doors
* All Ironmongery to match existing or similar.
* Double glazed panels to be used within door.
* All wooden door frames are to be taken from the solid and rebated and shaped to the profiles indicated on the drawings. All edges to be pencil rounded.
* Adhesives - Complying with BS 1204 : Part 1 and 2. Use external (type WPB) where applicable.
* Workmanship generally to conform to BS 1186 : Part 2.
* Finished wooden door frames are to be screw/plug and pellet fixed to block work/concrete walls only after completion of relating wall and floor finishes.

**Notes/Other**

* Timber finish to be dull gloss white to match existing/surrounding windows & doors.
* Local FENSA Approved contractor to be used for installation process.