|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Type | Measurements | Supplier | Drawings |
| Stone Front Steps | Portland Stone | To match existing | Portland Stone | Photo provided |
| Front Door | Hardwood with hardwood and glass fanlight to match existing | To match existing masonry openings | Broadleaf Timber | Drawings provided |
| Sash Windows - Georgian | Hardwood double glazed sash windows to match existing details and profiles | To match existing masonry openings | Bespoke | Drawings provided |
| Conservation Skylight | Conservation skylight | 2000mm x 2200mm | BD Bespoke Glazing | Drawings provided |
| Rear French doors and windows | Hardwood double glazed | See drawings | Vale Garden Houses | Drawings provided |