**Maintenance**

Maintenance of a green roof is paramount in order for the it to continue to offer aesthetic and environmental benefit to a building. All green roofs and walls will require some form of maintenance in order for the area to flourish for many years with a minimum of two inspections a year to ensure that the outlets etc are maintained.

To avoid unnecessary and sometimes costly remedial works in the future it is important for to carry out maintenance on a regular basis with the number of visits dependant on the planting scheme of the roof.

**Intensive green roof**

An intensive green roof will require the regular maintenance associated with the planting scheme and landscape design.

**Extensive green roof**

An extensive green roof will need only minimal maintenance to ensure that any unwanted species do not become established. We recommend a minimum of 2 visits per year.

**Services provided during maintenance**

Full roof evaluation with a comprehensive review of your green roof to determine any remedial work that could possibly be required

Full removal of unwanted items including leaves, debris and unwanted vegetation.

Full inspection of all roof outlets and removal of any encroaching vegetation to enable water to flow freely through rainwater pipes.

Full application of organic fertiliser to renew and restore the vegetation and encourage growth if required.

If there is one fitted - full testing of the irrigation system to make sure that everything is working as expected.