|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Element** | **Location** | **Sample or As R5N** | **Approved by Camden** |
| 1 | Brickwork – Selected Dark Facing | East, west and south elevations | As per R5 North |  |
| 2 | Brickwork – Mixture of Throckley Smooth Grey + Himley Ash Grey | North elevation | Sample panel located on site |  |
| 3 | St Joris Sawtooth glazed bricks | East and west elevations | As per R5 North |  |
| 4 | St Joris glazed sills and specials | East, west and south elevations | As per R5 North |  |
| 5 | St Joris glazed sills and specials | North elevation | As per R5 North South façade air bricks |  |
| 6 | Precast concrete element | Coping to roof and 8th floor terrace, window sills and ground floor curtain walling surround on all elevations | Colour As per sample |  |
| 7 | Aluminium windows and door systems by Schucco – Colour Anoline C34 | East, west and south elevations | Corner Sample available on site |  |
| 8 | Aluminium windows and door systems by Schucco – Colour Anoline C33 | North elevation | Corner Sample available on site |  |
| 9 | Aluminium soffit to match window colour | All elevations | To match window colour |  |
| 10 | Aluminium flashing to match window colour | East, west and south elevations | To match window colour |  |
| 11 | Curtain walling systems by Schucco – RAL colour 9019 | Ground floor to commercial and residential areas | Sample located on site |  |
| 12 | Sunray Steel doors – RAL colour 9019 | Ground floor east elevation substation | Sunray door in accordance with Metropolitan’s requirements |  |
| 13 | External aluminium rainwater pipes – RAL colour 8019 | North and east elevations |  |  |
| 14 | Architectural metalwork (zig-zag balusters) – RAL colour 8019 | East, west and south elevations | As per R5 North |  |
| 15 | Archtiectural metalwork (straight balusters) - RAL colour 8019 | North elevation and 1st floor terrace to East and west elevations | As per R5 North |  |
| 16 | Concealed shop fitted folding arm awning. Facia panel to match curtain walling. | West and south elevations | Fabric Sample on site |  |