**Balcony**

**Flat 3, 154 Iverson Road NW6 2HH**

**Privacy screen:**

Battens to be used: Western Red Cedar Slatted Screen Battens 19 x 38mm.

[http://www.silvatimber.co.uk/western-red-cedar-slatted-screen-battens-19x38mm.html](https://owa.nexus.ox.ac.uk/owa/redir.aspx?SURL=NG2IUvZ3IftlN8BsQsJoFU_HoZLUBsBJkor8XO2UcgEbFwe-jXbUCGgAdAB0AHAAOgAvAC8AdwB3AHcALgBzAGkAbAB2AGEAdABpAG0AYgBlAHIALgBjAG8ALgB1AGsALwB3AGUAcwB0AGUAcgBuAC0AcgBlAGQALQBjAGUAZABhAHIALQBzAGwAYQB0AHQAZQBkAC0AcwBjAHIAZQBlAG4ALQBiAGEAdAB0AGUAbgBzAC0AMQA5AHgAMwA4AG0AbQAuAGgAdABtAGwA&URL=http%3a%2f%2fwww.silvatimber.co.uk%2fwestern-red-cedar-slatted-screen-battens-19x38mm.html)

Sample photograph on the left below.



Steel frame: Black hand painted steel tube 20mm x 20mm x 2mm square hollow sections with side plate – Grade S235. Sample photograph on the right above.

**Balustrade**

* Colour: Black, Material: Metal Spindle - Metal Brackets & Rails, Height: 1100 mm,
* Post centres: 60mm. Sample photograph below.

