**Construction Management**

**Plan**

**pro forma** v2.2

**Contents**

**Revisions 3**

**Introduction 4**

**Timeframe 6**

[**Contact**](#_Contact) **7**

[**Site**](#_Site) **9**

[**Community liaison**](#_Community_Liaison) **12**

[**Transport**](#_Transport) **15**

[**Environment**](#_Environment) **25**

[**Agreement**](#_Agreement)  **30**

# Revisions & additional material

Please list all iterations here:

|  |  |  |
| --- | --- | --- |
| **Date** | **Version** | **Produced by** |
| **5th March 2018** | **Pro Forma v2.2** | **J K Puddy** **London Basement** |
| **26th June 2018** | **Pro Forma v2.2** | **J K Puddy** **London Basement** |

**Additional sheets**

Please note – the review process will be quicker if these are submitted as Word documents or searchable PDFs.

|  |  |  |
| --- | --- | --- |
| **Date** | **Version** | **Produced by** |
| **March 2017** | **Construction Management Plan** | **London Basement** |
| **January 17** | **Block Plan 1701/BL.02** | **Sher & White Architects** |
| **March 2017** | **16-027-SITE BLOCK PLAN** | **Basement Design Studio** |
| **March 2017** | **16-027-SITE PLAN** | **Basement Design Studio** |
| **June 2018** | **Construction Programme** | **London Basement** |
| **June 18** | **Plant Usage Table**  | **London Basement** |
| **June 18**  | **LB Waste Dust Noise and Vibration Policy** | **London Basement** |
| **June 18** | **CLOCS Compliance Diagram & Poster** | **UK.GOV** |
| **June 18** | **London Basement - Pest Service Agreement - June 2018** | **Rentokil** |
| **June 18**  | **London Basement – NVDMP Rev 1 June 18** | **London Basement** |

# Introduction

The purpose of the **Construction Management Plan (CMP)** is to help developers to minimise construction impacts, and relates to both on site activity and the transport arrangements for vehicles servicing the site.

It is intended to be a live document whereby different stages will be completed and submitted for application as the development progresses.

The completed and signed CMP must address the way in which any impacts associated with the proposed works, and any **cumulative impacts of other nearby construction sites**, will be mitigated and managed. The level of detail required in a CMP will depend on the scale and kind of development. Further policy guidance is set out in Camden Planning Guidance [**(CPG)** 6: Amenity](http://www.camden.gov.uk/ccm/content/environment/planning-and-built-environment/two/planning-policy/supplementary-planning-documents/camden-planning-guidance.en) and [**(CPG)** 8: Planning Obligations](http://www.camden.gov.uk/ccm/content/environment/planning-and-built-environment/two/planning-policy/supplementary-planning-documents/camden-planning-guidance.en).

This CMP follows the best practice guidelines as described in [Transport for London’s](https://www.tfl.gov.uk/info-for/freight/safety-and-the-environment/improving-construction-safety) (TfL’s Standard for [Construction Logistics and Community Safety](http://www.clocs.org.uk/standard-for-clocs/) (**CLOCS**) scheme) and [Camden’s Minimum Requirements for Building Construction](http://www.camden.gov.uk/ccm/cms-service/download/asset?asset_id=3257318) **(CMRBC)**.

The approved contents of this CMP must be complied with unless otherwise agreed with the Council in writing. The project manager shall work with the Council to review this CMP if problems arise in relation to the construction of the development. Any future revised plan must also be approved by the Council and complied with thereafter.

It should be noted that any agreed CMPdoes not prejudice or override the need to obtain any separate consents or approvals such as for road closures or hoarding licences.

If your scheme involves any demolition, you need to make an application to the Council’s Building Control Service. Please complete the “[**Demolition Notice**](http://www.camden.gov.uk/ccm/content/environment/building-control/file-storage-items/demolition-notice---the-building-act-1984-section-80-notice-bc104-.en)**.**”

Please complete the questions below with additional sheets, drawings and plans as required. The boxes will expand to accommodate the information provided, so please provide as much information as is necessary. **It is preferable if this document, and all additional documents, are completed electronically and submitted as Word files to allow comments to be easily documented. These should be clearly referenced/linked to from the CMP.**

Please notify that council when you intend to start work on site. Please also notify the council when works are approximately **3 months from completion.**

(Note the term 'vehicles' used in this document refers to all vehicles associated with the implementation of the development, e.g. demolition, site clearance, delivery of plant & materials, construction, etc.)

Revisions to this document may take place periodically.Timeframe

**DEVELOPER ACTIONS**

**COUNCIL ACTIONS**

**Post app submission**

**0ommunity liaison**

**Appoint principal contractor**

**Requirement to submit CMP**

**Begin community liaison**

**Council response to second draft**

**Work can commence if draft CMP is approved**

**Resubmission of CMP if first draft refused**

**2ommunity liaison**

**3ommunity liaison**

**1ommunity liaison**

INDICATIVE TIMEFRAME (MONTHS)

**4ommunity liaison**

**Council response to draft**

**Submit draft CMP**

# Contact

1. Please provide the full postal address of the site and the planning reference relating to the construction works.

Address:

Planning reference number to which the CMP applies:

2. Please provide contact details for the person responsible for submitting the CMP.

Name: Mr J K Puddy

Address: London Basement, Unit 4, Victory Business Centre, Fleming Way, Isleworth, TW7 6DB

Email: jake.puddy@londonbasement.co.uk

Phone: 020 8847 9449

3. Please provide full contact details of the site project manager responsible for day-to-day management of the works and dealing with any complaints from local residents and businesses.

Name: Mr J Zefi

Address: London Basement, Unit 4, Victory Business Centre, Fleming Way, Isleworth, TW7 6DB

Email: joe.zefi@londonbasement.co.uk

Phone: 020 8847 9449

4. Please provide full contact details of the person responsible for community liaison and dealing with any complaints from local residents and businesses if different from question 3. In the case of [**Community Investment Programme (CIP)**](http://www.camden.gov.uk/ccm/content/environment/planning-and-built-environment/two/placeshaping/twocolumn/the-community-investment-programme.en), please provide contact details of the Camden officer responsible.

Name: Mr J Zefi

Address: London Basement, Unit 4, Victory Business Centre, Fleming Way, Isleworth, TW7 6DB

Email: joe.zefi@londonbasement.co.uk

Phone: 020 8847 9449

5. Please provide full contact details including the address where the main contractor accepts receipt of legal documents for the person responsible for the implementation of the CMP.

Name: Mr K Birrane

Address: London Basement, Unit 4, Victory Business Centre, Fleming Way, Isleworth, TW7 6DB

Email: kenneth@londonbasement.co.uk

Phone: 020 8847 9449

# Site

6. Please provide a site location plan and a brief description of the site, surrounding area and development proposals for which the CMP applies.

See attached Block Plan 1701/BL.02

* 31 St Mark’s Crescent is a brick built, timber framed, semi-detached period property sited on St Marks Crescent which is in a residential area with two-way traffic. The property backs onto the Regents Canal.
* The proposed development involves the Excavation of a basement extension to single-family dwelling (Use Class C3) including no.1 rear lightwell and associated alterations to rear garden level.

7. Please provide a very brief description of the construction works including the size and nature of the development and details of the main issues and challenges (e.g. narrow streets, close proximity to residential dwellings etc).

The proposed works involve excavation, underpinning, installation of steel beams and columns with associated waterproofing and drainage works.

Access to the property for both site operatives and material deliveries are planned through the front entrance on St Marks Crescent. It is planned to utilise the Regents Canal for spoil removal.

8. Please identify the nearest potential receptors (dwellings, business, etc.) likely to be affected by the activities on site (i.e. noise, vibration, dust, fumes, lighting etc.).

**57 Gloucester Ave – Freeholder and 4 no leaseholders:**

**59 Gloucester Ave – Freeholder**

**1 St Mark’s Crescent – Freeholder**

9. Please provide a scaled plan detailing the local highway network layout in the vicinity of the site. This should include details of on-street parking bay locations, cycle lanes, footway extents and proposed site access locations.

Please see attached Block Plan 1701/BL.02, 16-027-SITE BLOCK PLAN and 16-027-SITE PLAN

10. Please provide the proposed start and end dates for each phase of construction as well as an overall programme timescale. (A Gantt chart with key tasks, durations and milestones would be ideal).

Please see attached document - Draft Construction Programme

11. Please confirm the standard working hours for the site, noting that the standard working hours for construction sites in Camden are as follows:

* 8.00am to 6pm on Monday to Friday
* 8.00am to 1.00pm on Saturdays
* No working on Sundays or Public Holidays

Working hours will be from 0800 to 1800 Monday to Friday and 0800 to 1300 on Saturdays. There will be no working on Sundays or Public Holidays.

12. Please indicate if any changes to services are proposed to be carried out that would be linked to the site during the works (i.e. connections to public utilities and/or statutory undertakers’ plant). Larger developments may require new utility services. If so, a strategy and programme for coordinating the connection of services will be required. If new utility services are required, please confirm which utility companies have been contacted (e.g. Thames Water, National Grid, EDF Energy, BT etc.) You must explore options for the utility companies to share the same excavations and traffic management proposals. Please supply details of your discussions.

It is not proposed that any changes to services will be required.

# Community Liaison

**A neighbourhood consultation process must have been undertaken prior to submission of the CMP first draft. This consultation must relate to construction impacts, and should take place following the granting of planning permission in the lead up to the submission of the CMP. A consultation process specifically relating to construction impacts must take place regardless of any prior consultations relating to planning matters. This consultation must include all of those individuals that stand to be affected by the proposed construction works. These individuals should be provided with a copy of the draft CMP, or a link to an online document. They should be given adequate time with which to respond to the draft CMP, and any subsequent amended drafts. Contact details which include a phone number and email address of the site manager should also be provided.**

Significant time savings can be made by running an effective neighbourhood consultation process. This must be undertaken in the spirit of cooperation rather than one that is dictatorial and unsympathetic to the wellbeing of local residents and businesses.

These are most effective when initiated as early as possible and conducted in a manner that involves the local community. Involving locals in the discussion and decision making process helps with their understanding of what is being proposed in terms of the development process. **The consultation and discussion process should have already started, with the results incorporated into the CMP first draft submitted to the Council for discussion and sign off.**This communication should then be ongoing during the works, with neighbours and any community liaison groups being regularly updated with programmed works and any changes that may occur due to unforeseen circumstances through newsletters, emails and meetings.

Please note that for larger sites, details of a construction working group may be required as a separate S106 obligation. If this is necessary, it will be set out in the S106 Agreement as a separate requirement on the developer.

**Cumulative impact**

Sites located within high concentrations of construction activity that will attract large numbers of vehicle movements and/or generate significant sustained noise levels should consider establishing contact with other sites in the vicinity in order to manage these impacts.

**The Council can advise on this if necessary.**

**13. Consultation**

The Council expects meaningful consultation. For large sites, this may mean two or more meetings with local residents **prior to submission of the first draft CMP**.

Evidence of who was consulted, how the consultation was conducted and a summary of the comments received in response to the consultation should be included. Details of meetings including minutes, lists of attendees etc. should be appended.

In response to the comments received, the CMP should then be amended where appropriate and, where not appropriate, a reason given. The revised CMP should also include a list of all the comments received. Developers are advised to check proposed approaches to consultation with the Council before carrying them out. If your site is on the boundary between boroughs then we would recommend contacting the relevant neighbouring planning authority.

Please provide details of consultation of draft CMP with local residents, businesses, local groups (e.g. residents/tenants and business associations) and Ward Councillors.

The immediate neighbours have been consulted throughout the party wall and planning process, whilst various addressees requested copies of the CMP or acknowledged receipt, no parties have made any comment on the proposals, notification of the plans was issued to all residents on St Marks Crescent at planning stage and the Draft Construction Management Plan was approved within the DDN and Sect 106 agreement. London Basement have engaged with the Canals & Rivers Trust also and have their written consent for the planned spoil removal methodology.

**14. Construction Working Group**

Please provide details of community liaison proposals including any Construction Working Group that will be set up, addressing the concerns of the community affected by the works, the way in which the contact details of the person responsible for community liaison will be advertised to the local community, and how the community will be updated on the upcoming works i.e. in the form of a newsletter/letter drop, or weekly drop in sessions for residents.

Prior to commencement onsite the Contractor will undertake to notify by letter all residents with 500m of the site in either direction and on both sides of St. Marks Crescent. This letter will contain details of the anticipated duration of the project, the agreed working hours of the site and the contact details of the Head Office, the Supervisory Staff and Health & Safety Officers.

The Contractor will also provide a regular newsletter to local resident to update them on progress and measures taken to protect their interests.

The Contractor will answer any queries in a timely fashion and endeavour to take all feedback into consideration throughout the full programme of works.

**15. Schemes**

Please provide details of your ‘Considerate Constructors Scheme’ registration, and details of any other similar relevant schemes as appropriate. Contractors will also be required to follow the “[Guide for Contractors Working in Camden](http://www.camden.gov.uk/ccm/cms-service/download/asset?asset_id=799001)” also referred to as “[Camden’s Considerate Contractors Manual](http://www.camden.gov.uk/ccm/cms-service/download/asset?asset_id=799001)”.

London Basement is registered with the Considerate Constructors Scheme and always works within its guidelines. We have also reviewed the Guide for Contractors Working in Camden and its contents has been considered in preparing this Construction Management Plan.

**16. Neighbouring sites**

Please provide a plan of existing or anticipated construction sites in the local area and please state how your CMP takes into consideration and mitigates the cumulative impacts of construction in the vicinity of the site. The council can advise on this if necessary.

Please refer to section 2 in the attached document - Construction Management Plan

# Transport

**This section must be completed in conjunction with your principal contractor. If one is not yet assigned, please leave the relevant sections blank until such time when one has been appointed.**

Camden is a CLOCS Champion, and is committed to maximising road safety for Vulnerable Road Users (VRUs) as well as minimising negative environmental impacts created by motorised road traffic. As such, all vehicles and their drivers servicing construction sites within the borough are bound by the conditions laid out in the [CLOCS Standard.](http://www.clocs.org.uk/)

This section requires details of the way in which you intend to manage traffic servicing your site, including your road safety obligations with regard to VRU safety. It is your responsibility to ensure that your principal contractor is fully compliant with the terms laid out in the CLOCS Standard. It is your principal contractor’s responsibility to ensure that all contractors and sub-contractors attending site are compliant with the terms laid out in the CLOCS Standard.

Checks of the proposed measures will be carried out by the council to ensure compliance. Please refer to the CLOCS Standard when completing this section. Guidance material which details CLOCS requirements can be accessed [here](http://www.camden.gov.uk/ccm/cms-service/stream/asset?asset_id=3550016&), details of the monitoring process are available [here](http://www.camden.gov.uk/ccm/cms-service/stream/asset?asset_id=3550014&).

Please contact CLOCS@camden.gov.uk for further advice or guidance on any aspect of this section.

**Please refer to the CLOCS Overview and Monitoring Overview documents referenced above which give a breakdown of requirements.**

**CLOCS Contractual Considerations**

17. Name of Principal contractor:

London Basement

18. Please submit the proposed method for checking operational, vehicle and driver compliance with the CLOCS Standard throughout the duration of the contract (please refer to our [CLOCS Overview document](http://www.camden.gov.uk/ccm/cms-service/stream/asset?asset_id=3550016&) and [Q18 example response](http://www.camden.gov.uk/ccm/cms-service/stream/asset?asset_id=3550015&)).

London Basement does not operate its own fleet and relies upon sub-contractor supplies and deliveries, the muck away which is typically the primary source of vehicle movement for this kind of work has been taken off the road and is being moved by barge.

The remainder of site traffic is therefore deliveries of steel, bagged concrete materials and sundry items for which we only use 2 main suppliers both of whom are accredited FORS Silver Standard with our main supplier Ashville Inc. being Gold Standard, as part of this accreditation and in order to progress from Bronze to Silver all drivers must have completed 1 safety related e-learning module plus a Van Smart course, a On-Cycle training and Safe Urban Driver training. Further details of our suppliers membership can be found here <https://www.fors-online.org.uk/cms/whos-on-board/>

London Basement will at point of order ensure through written assurance that all supply and muck away contractors using vehicles over 3.5T are registered with FORS using the CLOCS Compliance check form and non-conformance report form. Non-conforming vehicles or operators will not be considered for employment.

All vehicles attending site over 3.5T will be required to have blindspot minimisation equipment and audible left turn alerts

Site managers will be issued with Compliance checking and monitoring process-diagram

* The site will display the CLOCS compliance poster A1 size in a prominent place on the site hoarding. (see Additional Sheets )

19. Please confirm that you as the client/developer and your principal contractor have read and understood the [CLOCS Standard](http://www.clocs.org.uk/wp-content/uploads/2015/05/CLOCS-Standard-v1.2-APRIL_15.pdf) and included it in your contracts. Please sign-up to join the [CLOCS Community](http://www.clocs.org.uk/links-to-partners/) to receive up to date information on the standard by expressing an interest online.

I confirm that I have included the requirement to abide by the CLOCS Standard in my contracts to my contractors and suppliers:

Confirmed

Please contact CLOCS@camden.gov.uk for further advice or guidance on any aspect of this section.

**Site Traffic**

**Sections below shown in blue directly reference the CLOCS Standard requirements. The CLOCS Standard should be read in conjunction with this section.**

**20. Traffic routing**: *“Clients shall ensure that a suitable, risk assessed vehicle route to the site is specified and that the route is communicated to all contractors and drivers. Clients shall make contractors and any other service suppliers aware that they are to use these routes at all times unless unavoidable diversions occur.”* (P19, 3.4.5)

Routes should be carefully considered and risk assessed, taking into account the need to avoid where possible any major cycle routes and trip generators such as schools, offices, public buildings,museums etc. Where appropriate, on routes that use high risk junctions (i.e. those that attract high volumes of cycling traffic) installing Trixi mirrors to aid driver visibility should be considered.

Consideration should also be given to weight restrictions, low bridges and cumulative impacts of construction (including neighbouring construction sites) on the public highway network. The route(s) to and from the site should be suitable for the size of vehicles that are to be used.

a. Please indicate routes on a drawing or diagram showing the public highway network in the vicinity of the site including details of how vehicles will be routed to the [Transport for London Road Network](http://www.lscp.org.uk/lrsu/engineering_tlrn.html) (TLRN) on approach and departure from the site.

Please see Appendix 3 of the attached Construction Management Plan – Routes & Directions.

b. Please confirm how contractors, delivery companies and visitors will be made aware of the route (to and from the site) and of any on-site restrictions, prior to undertaking journeys.

Contractors, delivery companies and visitors will be made aware of the route and that there is no parking available on site. All site operatives are encouraged to use public transport and a copy of the CMP will be kept on site for reference. The CMP will also be attached to all primary purchase orders thus alerting delivery companies to the route. The foreman will ensure that drivers adhere to this and should any driver fail to follow the route and direction their head office will be advised and asked to take remedial action.

**21. Control of site traffic, particularly at peak hours**: “*Clients shall consider other options to plan and control vehicles and reduce peak hour deliveries”* (P20, 3.4.6)

Construction vehicle movements are generally acceptable between 9.30am to 4.30pm on weekdays and between 8.00am and 1.00pm on Saturdays). If there is a school in the vicinity of the site or on the proposed access and/or egress routes, then deliveries must be restricted to between 9.30am and 3pm on weekdays during term time. (Refer to the [*Guide for Contractors Working in Camden*](http://www.camden.gov.uk/ccm/cms-service/download/asset?asset_id=799001)).

A delivery plan should ensure that deliveries arrive at the correct part of site at the correct time. Instructions explaining such a plan should be sent to all suppliers and contractors**.** Consideration should be given to the location of any necessary holding areas for large sites with high volumes of traffic. Vehicles must not wait or circulate on the public highway. Whilst deliveries should be given set times to arrive, dwell and depart, no undue time pressures should be placed upon the driver at any time.

a. Please provide details of the typical sizes of all vehicles and the approximate frequency and times of day when they will need access to the site, for each phase of construction.You should estimate the average daily number of vehicles during each major phase of the work, including their dwell time at the site. High numbers of vehicles per day and/or long dwell times may require vehicle holding procedures.

|  |  |
| --- | --- |
| **Vehicle type/no of visits per day**  | **Dimensions** |
| 1 staff van/day maximum  | 5.6m x 2.1m |
| 1 material delivery/day maximum | 7.5m x 2.45m |

b. Please provide details of other developments in the local area or on the route.

c. Please outline the system that is to be used to ensure that the correct vehicle attends the correct part of site at the correct time.

All deliveries will be to the front of the site

As there are schools within the immediate vicinity of the site construction vehicle movements will be restricted to between 10.00 and 15.30 Monday to Friday.

A map of the route construction vehicles should take will be attached to purchase orders. London Basement follows a strict call off procedure detailed as follows:

**London Basement Call Off Procedure**

1. Materials will be ordered through the Head Office Purchasing Department at least 48 hours prior to their requirement onsite. Site foremen will be instructed to ensure orders are to be kept to a minimum to avoid delays in off load and double handling after being stored in our compound.

2. We use licensed contractors for the removal of our excavated material, which will be requested by site staff and scheduled by the Head Office Contracts Administrator a minimum of 24 hours prior to their requirement on site.

3. All delivery/collection drivers will be required to notify the site foreman at least 20 minutes before arrival.

4. All deliveries/collections will be arranged for between 10.00 and 15.30 Monday to Friday. Any deliveries/collections out of the stipulated time boundaries will be refused.

5. Stacking of vehicles is not acceptable at any time.

d. Please identify the locations of any off-site holding areas (an appropriate location outside the borough may need to be identified, particularly if a large number of delivery vehicles are expected) and any measures that will be taken to ensure the prompt admission of vehicles to site in light of time required for any vehicle/driver compliance checks. Please refer to question 24 if any parking bay suspensions will be required for the holding area.

This is a residential extension project and large numbers of delivery vehicles are not expected. There will be no requirement for off-site holding areas. There will be no double stacking of vehicles attending site and this will be managed through the London Basement call off procedure. Vehicles attending site outside of their allocated times will be sent away.

e. Please provide details of any other measures designed to reduce the impact of associated traffic (such as the use of [construction material consolidation centres](https://www.google.co.uk/url?sa=t&rct=j&q=&esrc=s&source=web&cd=2&cad=rja&uact=8&ved=0ahUKEwi5hKjPiLjRAhVqLcAKHQduC_gQFggkMAE&url=http%3A%2F%2Fcontent.tfl.gov.uk%2Fdirectory-london-construction-consolidation-centres.pdf&usg=AFQjCNFhB34aaqw3M3fmDpJYUUBw_PjbdA&sig2=KXhGnTR3slzf0kN4XMOcQg&bvm=bv.143423383,d.ZWM)).

Site operatives are encouraged to use public transport to get to work. By using the canal for muck away by barge we will minimise the volume of vehicular traffic. All materials will be stored on site therefore consolidation centres will not be required.

**22. Site access and egress:** “*Clients shall ensure that access to and egress from the site is appropriately managed, clearly marked, understood and clear of obstacles.”* (P18, 3.4.3)

Vehicles entering and leaving the site should be carefully managed, using gates that are clearly marked and free from obstacles. Traffic marshals must ensure the safe passage of all traffic on the public highway, in particular pedestrians and cyclists, when vehicles are entering and leaving site, particularly if reversing.

Traffic marshals, or site staff acting as traffic marshals, should hold the relevant qualifications required for directing large vehicles when reversing. Marshals should be equipped with ‘STOP – WORKS’ signs (not STOP/GO signs) if control of traffic on the public highway is required. Marshals should have radio contact with one another where necessary.

a. Please detail the proposed access and egress routes to and from the site

This is a pedestrian site and no vehicles will enter or leave the site compound.

b. Please describe how the access and egress arrangements for construction vehicles will be managed.

Although no vehicles will have access to or egress from site fully trained banksmen will be in attendance as necessary for all deliveries and collections.

c. Please provide swept path drawings for any tight manoeuvres on vehicle routes to and from the site including proposed access and egress arrangements at the site boundary (if necessary).

There are no tight manoeuvres on the proposed routes to and from site. There will be no vehicle access to or egress from the site.

d. Provision of wheel washing facilities should be considered if necessary. If so, please provide details of how this will be managed and any run-off controlled.

This is a pedestrian site with no vehicle access, so wheel washing facilities will not be required.

**23. Vehicle loading and unloading:** *“Clients shall ensure that vehicles are loaded and unloaded on-site as far as is practicable.”* (P19, 3.4.4)

If this is not possible, Traffic Marshalls must ensure the safe passage of pedestrians, cyclists and motor traffic in the street when vehicles are being loaded or unloaded.

Please provide details of the parking and loading arrangements for construction vehicles with regard to servicing and deliveries associated with the site (e.g. delivery of materials and plant, removal of excavated material). This is required as a scaled site plan, showing all points of access and where materials, skips and plant will be stored, and how vehicles will access and egress the site. If loading is to take place off site, please identify where this is due to take place and outline the measures you will take to ensure that loading/unloading is carried out safely. Please outline in question 24 if any parking bay suspensions will be required.

The site will have no vehicle access. All deliveries and collections will take place on the street. Trained banksmen will be in attendance throughout and priority given to pedestrians and other road users. Deliveries will be immediately taken into the site itself and not stored on the highway. Parking bay suspensions will be required as detailed below.

**Highway interventions**

**Please note that Temporary Traffic Orders (TTOs) and hoarding/scaffolding licenses may be applied for prior to CMP submission but won’t be granted until the CMP is signed-off.**

**If the site is on or adjacent to the TLRN, please provide details of preliminary discussions with Transport for London in the relevant sections below.**

**24. Parking bay suspensions and temporary traffic orders**

Please note, parking bay suspensions should only be requested where absolutely necessary. Parking bay suspensions are permitted for a maximum of 6 months, requirement of exclusive access to a bay for longer than 6 months you will be required to obtain [Temporary Traffic Order (TTO)](http://camden.gov.uk/ccm/content/transport-and-streets/traffic-management/temporary-road-restrictions/) for which there is a separate cost.

Please provide details of any proposed parking bay suspensions and TTO’s which would be required to facilitate construction. **Building materials and equipment must not cause obstructions on the highway as per your Considerate Contractors obligations unless the requisite permissions are secured.**

Information regarding parking suspensions can be found [here.](http://www.camden.gov.uk/ccm/navigation/transport-and-streets/parking/parking-bay-suspensions/)

 We confirm the length will be limited to 1 bay for offload only , the suspension will not be required for the entire duration of the programmed works and it is not expected that a TTO will be required

**25. Scaled drawings of highway works**

Please note that use of the public highway for storage, site accommodation or welfare facilities is at the discretion of the Council and is generally not permitted. If you propose such use you must supply full justification, setting out why it is impossible to allocate space on-site. You must submit a detailed (to-scale) plan showing the impact on the public highway that includes the extent of any hoarding, pedestrian routes, parking bay suspensions and remaining road width for vehicle movements. We prefer not to close footways but if this is unavoidable, you should submit a scaled plan of the proposed diversion route showing key dimensions.

a. Please provide accurate scaled drawings of any highway works necessary to enable construction to take place (e.g. construction of temporary vehicular accesses).

No highway works will be needed or are planned.

b.Please provide details of all safety signage, barriers and accessibility measures such as ramps and lighting etc.

Please refer to 16-027 Site Plan for details

**26. Diversions**

Where applicable, please supply details of any diversion, disruption or other anticipated use of the public highway during the construction period (alternatively a plan may be submitted).

No diversions, disruptions or other uses of the public highway during the construction period are anticipated.

**27. VRU and pedestrian diversions, scaffolding and hoarding**

Pedestrians and/or cyclist safety must be maintained if diversions are put in place. Vulnerable footway users should also be considered. These include wheelchair users, the elderly, those with walking difficulties, young children, those with prams, the blind and partially sighted. Appropriate ramping must be used if cables, hoses, etc. are run across the footway.

Any work above ground floor level may require a covered walkway adjacent to the site. A licence must be obtained for scaffolding and gantries. The adjoining public highway must be kept clean and free from obstructions. Lighting and signage should be used on temporary structures/skips/hoardings etc.

A secure hoarding will generally be required at the site boundary with a lockable access.

a. Please provide details describing how pedestrian and cyclist safety will be maintained, including any proposed alternative routes (if necessary), and any Traffic Marshall arrangements.

Pedestrian and cyclist safety will be maintained at all times of site operation. Site operatives will be under a standing instruction to ensure pedestrian traffic is not limited by the works and care will be taken to ensure materials being carried into the site do not block pedestrian traffic. Trained banksmen will be present as required when construction vehicles are in attendance to supervise deliveries and collections.

b. Please provide details of any temporary structures which would overhang the public highway (e.g. scaffolding, gantries, cranes etc.) and details of hoarding requirements or any other occupation of the public highway.

No structures overhang the public highway, please refer to 16-027 Site Plan for details

SYMBOL IS FOR INTERNAL USE

# Environment

To answer these sections please refer to the relevant sections of **Camden’s Minimum Requirements for Building Construction (**[**CMRBC**](http://www.camden.gov.uk/ccm/cms-service/download/asset?asset_id=3257318)**).**

28. Please list all [noisy operations](http://www.camden.gov.uk/ccm/content/environment/environmental-health--consumer-protection/noise/reducing-noise/noise-from-construction-sites.en?page=2)  and the construction method used, and provide details of the times that each of these are due to be carried out.

Please see attached document - table 1. plant usage

These works will be carried out between 0800 and 1700

29. Please confirm when the most recent noise survey was carried out (before any works were carried out) and provide a copy. If a noise survey has not taken place please indicate the date (before any works are being carried out) that the noise survey will be taking place, and agree to provide a copy.

A noise survey has not been undertaken but will be carried out approximately 2 weeks before works start on site. A copy of this survey will be provided to the Local Authority for their records.

30. Please provide predictions for [noise](http://www.camden.gov.uk/ccm/content/environment/environmental-health--consumer-protection/noise/reducing-noise/noise-from-construction-sites.en?page=2) and vibration levels throughout the proposed works.

Please see attached document - table 1. plant usage

31. Please provide details describing mitigation measures to be incorporated during the construction/[demolition](http://www.camden.gov.uk/ccm/navigation/environment/building-control/demolition/) works to prevent noise and vibration disturbances from the activities on the site, including the actions to be taken in cases where these exceed the predicted levels.

Please see attached document LB Waste Dust Noise and Vibration Policy

32. Please provide evidence that staff have been trained on BS 5228:2009

All staff receives ongoing training including regarding noise and vibration levels (BS 5228:2009). All site managers have taken the five-day Site Managers Safety Training Scheme (SMSTS) course. Individual certificates will be copied within the site compendium for inspection.

33. Please provide details on how dust nuisance arising from dusty activities, on site, will be prevented.

Please see attached document LB Waste Dust Noise and Vibration Policy

34. Please provide details describing how any significant amounts of dirt or dust that may be spread onto the public highway will be prevented and/or cleaned.

Please see attached document LB Waste Dust Noise and Vibration Policy

35. Please provide details describing arrangements for monitoring of [noise](http://www.camden.gov.uk/ccm/content/environment/environmental-health--consumer-protection/noise/reducing-noise/noise-from-construction-sites.en?page=2), vibration and dust levels.

Please see attached document LB Waste Dust Noise and Vibration Policy

36. Please confirm that a Risk Assessment has been undertaken at planning application stage in line with the GLA policy. [The Control of Dust and Emissions During Demolition and Construction 2104 (SPG)](https://www.london.gov.uk/file/18750/download?token=zV3ZKTpP), that the risk level that has been identified, and that the appropriate measures within the GLA mitigation measures checklist have been applied. Please attach the risk assessment and mitigation checklist as an appendix.

Please see attached document LB Waste Dust Noise and Vibration Policy

37. Please confirm that all of the GLA’s ‘highly recommended’ measures from the [SPG](https://www.london.gov.uk/file/18750/download?token=zV3ZKTpP) document relative to the level of risk identified in question 36 have been addressed by completing the [GLA mitigation measures checklist.](https://www.london.gov.uk/what-we-do/planning/implementing-london-plan/supplementary-planning-guidance/control-dust-and)

Confirmed

38. If the site is a ‘High Risk Site’, 4 real time dust monitors will be required. If the site is a ‘Medium Risk Site’, 2 real time dust monitors will be required. The risk assessment must take account of proximity to sensitive receptors (e.g. schools, care homes etc), as detailed in the [SPG](https://www.london.gov.uk/file/18750/download?token=zV3ZKTpP). Please confirm the location, number and specification of the monitors in line with the SPG and confirm that these will be installed 3 months prior to the commencement of works, and that real time data and quarterly reports will be provided to the Council detailing any exceedances of the threshold and measures that were implemented to address these.

N/A Low risk

39. Please provide details about how rodents, including [rats](http://www.camden.gov.uk/ccm/content/environment/environmental-health--consumer-protection/pest-control/about-the-pest-control-service.en), will be prevented from spreading out from the site. You are required to provide information about site inspections carried out and present copies of receipts (if work undertaken).

A pest control survey is booked for the 11th June 2018

40. Please confirm when an asbestos survey was carried out at the site and include the key findings.

An asbestos survey is booked for the 11th June 2018

41. Complaints often arise from the conduct of builders in an area. Please confirm steps being taken to minimise this e.g. provision of a suitable smoking area, tackling bad language and unnecessary shouting.

The works are contained within the site, welfare areas are contained within the site and London Basement operates a strict no smoking policy, all site supervisory staff are trained in the 5 day SMSTS and London Basement is a Siver Award winner in the Considerate Constructors Scheme ( evidence attached )

42. If you will be using non-road mobile machinery (NRMM) on site with net power between 37kW and 560kW it will be required to meet the standards set out below. The standards are applicable to both variable and constant speed engines and apply for both PM and NOx emissions.

**From 1st September 2015**

**(i) Major Development Sites** – NRMM used on the site of any major development will be required to meet Stage IIIA of EU Directive 97/68/EC

**(ii) Any development site within the Central Activity Zone -** NRMM used on any site within the Central Activity Zone will be required to meet Stage IIIB of EU Directive 97/68/EC

**From 1st September 2020**

**(iii) Any development site -** NRMM used on any site within Greater London will be required to meet Stage IIIB of EU Directive 97/68/EC

**(iv) Any development site within the Central Activity Zone -** NRMM used on any site within the Central Activity Zone will be required to meet Stage IV of EU Directive 97/68/EC

Please provide evidence demonstrating the above requirements will be met by answering the following questions:

1. Construction time period (07/18- 03/19 ):
2. Is the development within the CAZ? (Y/N): NO
3. Will the NRMM with net power between 37kW and 560kW meet the standards outlined above? (Y/N): YES
4. Please provide evidence to demonstrate that all relevant machinery will be registered on the NRMM Register, including the site name under which it has been registered: All relevant machinery will be registered on the NRMM Register and it will include the site name under which it has been registered, this will be within the site compendium and available for inspection.
5. Please confirm that an inventory of all NRMM will be kept on site and that all machinery will be regularly serviced and service logs kept on site for inspection: CONFIRMED
6. Please confirm that records will be kept on site which details proof of emission limits, including legible photographs of individual engine plates for all equipment, and that this documentation will be made available to local authority officers as required:

SYMBOL IS FOR INTERNAL USE

# Agreement

The agreed contents of this Construction Management Plan must be complied with unless otherwise agreed in writing by the Council. This may require the CMP to be revised by the Developer and reapproved by the Council. The project manager shall work with the Council to review this Construction Management Plan if problems arise in relation to the construction of the development. Any future revised plan must be approved by the Council in writing and complied with thereafter.

It should be noted that any agreed Construction Management Plan does not prejudice further agreements that may be required such as road closures or hoarding licences.

**Please notify that council when you intend to start work on site. Please also notify the council when works are approximately 3 months from completion.**

**Signed:**



**Date:** 5th June 2018

**Print Name:** J K Puddy

**Position:** Business Development

Please submit to: planningobligations@camden.gov.uk

End of form.