**Sedum Roof Maintenance Plan**

Maintenance to be provided at least twice a year

In the Spring, slow release Granular Fertiliser to be sprinkled onto the Sedum Roof

Sedum Roof to be watered regularly over the Summer

In the Autumn weeds and invasive/unwanted species to be cleared and removed

Outlets to be cleaned and kept clear