**Tree Statement**

A small Lime Tree of species Tilia Cordata Greenspire will be planted in the corner of the front garden, adjacent to the highway in accordance with BS8545:2014 – Trees from Nursery to independence in the landscape

The replacement tree will not be in a raised bed – the soil level of the front garden and the tree pit will be the same

The tree will be planted extra heavy standard 16-18cm in diameter measured at 1m in height

The tree pit 1.2m x 1.2m shall be excavated to a depth of at least 800mm

The tree will be back filled to 500mm with top soil

The pit will be backfilled with high quality top soil

The top 500mm will be high quality top soil

The tree will be suitably staked and tied

The base of the stem will be just below the surface of the soil

The tree pit will be clear of hard surfacing

The tree will be planted between November 2019 and March 2020