**Euronet Worldwide**

**Design and Access Statement for proposed installation of a replacement ATM to be installed as a Rear Loading Self Serv 26 ATM.**

**Cashpoint Currency Exchange 142 Southampton Row London WC1B 5AG**

**Introduction**

This Planning Statement has been prepared on behalf of Euronet Worldwide in support of an application submitted for the installation of a replacement Automated Teller Machine at 142 Southampton Row London. A NCR Self Serv 26 ATM is proposed to be installed through the left hand window frame, as a through glass installation, replacing the existing Cardtronics NCR ATM.

**The initial purpose of the proposal**

To continue to provide 24 hour banking facilities for customers of Cashpoint Currency Exchange 142 Southampton Row.

**Design Principles**

Proposed design is a NCR Self Serv 26 ATM fascia. Within the fascia is an acrylic standard NCR signage panel. This is illuminated and is to be fitted with Euronet ATM signage with blue lettering “ATM” out of a white background.

**Scale**

The dimensions of the installation are:-

ATM fascia to be set at a Height of 700 mm from the pavement level to the underside of the ATM fascia. ATM fascia Height 1109mm. Width 548mm.

The display screen is carefully shielded from ambient lighting to prevent glare and reflection, ensuring a clear and sharp image is visual by ATM customers.

**Appearance**

The proposed ATM is a standard NCR Self Serv 26 to be rear serviced within 142 Southampton Row.

The installation has been designed to anticipate and overcome the restriction that would prevent disabled persons from making full use of the service to be provided together with the needs of more vulnerable people from protection of attack and intimidation.

**Conclusion**

The proposed replacement ATM will continue to give the principal benefit to the community of providing cash on demand to customers of Cashpoint Currency Exchange 142 Southampton Row London WC1B 5AG